

#################### PYOTE 5.7.11  session started: Mon Dec  1 21:03:08 2025  ####################

filename: /home/nas/carsten/Polaris/Pictures/DVTI/Report/20251201_(2808) Belgrano/pyMovie.csv

==================== file header lines ====================
# PyMovie Version 4.1.5
# source: /home/nas/carsten/Polaris/Pictures/DVTI/Report/20251201_(2808) Belgrano/20251201_171215_408x310_G24dB_0050ms/20251201_171215_408x310_G24dB_0050ms.adv
#
# Aperture photometry was used to extract the lightcurves
#
# lunar background: False
# yellow mask = default: False
#
# aperture name: Target
# ____ aperture size: 21
# ____ x,y: (329, 154) at frame 1199
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: red
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 0
#
# aperture name: track
# ____ aperture size: 21
# ____ x,y: (162, 49) at frame 1199
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: yellow
# ____ joggable: False
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 1
#
# aperture name: empty
# ____ aperture size: 21
# ____ x,y: (297, 162) at frame 1199
# ____ threshold: 99999
# ____ def mask radius: 2.4
# ____ color: green
# ____ joggable: True
# ____ auto textOut: False
# ____ thumbnail source: False
# ____ csv output order: 2
#
# date at frame 0: 2025-12-01
#ACQUISITION-DELAY: 0.0
#ALTITUDE: 964.5
#AUTHOR: Carsten Ziolek
#BINNING-X: 4
#BINNING-Y: 4
#CAMERA-DRIVER-NAME: UVC
#CAMERA-FIRMWARE-VERSION: 1.3.2
#CAMERA-MODEL: DVTI+CAM
#CAMERA-SENSOR-INFO: Sony IMX430LLJ-C (9.2mm 1624x1240 4.5um CIS)
#CAMERA-SERIAL-NO: 43
#CAMERA-VENDOR-NAME: DVTI
#COMMENT: 
#DEC: 2.152504
#HEIGHT: 310
#INSTRUMENT: DVTI+CAM #43 FW 1.3.2, Sensor IMX430
#LATITUDE: 46.9925000
#LONGITUDE: 9.6400838
#OBJNAME: (2808) Belgrano occ. UCAC4 461-130431
#OBSERVER: Carsten Ziolek
#RA: 22.997271
#RECORDER-SOFTWARE: DvtiCamControl
#RECORDER-SOFTWARE-VERSION: 5.9.0-81
#TELESCOPE: C-14 EHD + 0.4x Red.
#WIDTH: 408
#
# Aperture photometry was used to extract the lightcurves
==================== end header lines ====================

No time step irregularities found.

timeDelta: 0.0499867 seconds per reading
timestamp error rate: 0.00%

Home directory: /home/carsten/.local/python-venv/lib/python3.10/site-packages/pyoteapp

We found /home/carsten/Documents/model-examples already present. Adding any new examples ...
signal-track is selected as the reference curve for normalization.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

signal-Target is the target curve.

Background region selected: [0, 526]

Background region selected: [685, 1199]

signal-Target is the light curve undergoing "selected points" noise analysis.
...This noise analysis uses 1042 points

noise corr coefs: [1.00, 0.0814]  (based on 1042 points)  sigmaB: 416.87

statistics of selected points:
...mean(selected points): 2941.23
...std(selected points) : 436.355
...std(detrended points): 416.868  (Warning: this sets sigmaB for the remainder of this session)
...baseline snr: 7.06  (using detrended std)

Background regions cleared.

signal-Target is the target curve.

Use min/max event to locate a "D and R" event has been selected

minEvent: 20  maxEvent: 40

Number of candidate solutions: 24549 (using event min/max entries)

New solver results...

Integer (non-subframe) solution...
B:2951.61  A:207.48
in entryNum units: D: 599  R: 627

noise corr coefs: [1.00, 0.0814]  (based on 1042 points)  sigmaB: 448.02

noise corr coefs: [1.00, 0.0814]  (based on 1042 points)  sigmaB: 448.02

Subframe adjusted solution...
B:2951.61  A:189.93
in entryNum units: D: 599  R: 627  D(subframe): 599.1727  R(subframe): 627.0000

in frameNum units: D: 599  R: 627  D(subframe): 599.1727  R(subframe): 627.0000

... end New solver results

signal-Target is the target curve.

Calculating the noise-induced-drop probability - this can take many seconds!  Be patient.

Error bar report based on 50,000 simulations (units are readings)...

loDbar   @ .68 ci:  -0.1146
hiDbar   @ .68 ci:   0.1242
loDbar   @ .95 ci:  -0.2862
hiDbar   @ .95 ci:   0.2656
loDbar   @ .9973 ci:  -0.5324
hiDbar   @ .9973 ci:   0.5506

loDurBar @ .68 ci:  -0.1791
hiDurBar @ .68 ci:   0.1782
loDurBar @ .95 ci:  -0.3929
hiDurBar @ .95 ci:   0.3877
loDurBar @ .9973 ci:  -0.7111
hiDurBar @ .9973 ci:   0.6800

Timestamp validity check ...

From timestamps at D and R, calculated 28 reading blocks.  From reading blocks, calculated 28 blocks.

Timestamps appear valid @ D and R

================= 0.68 containment interval report =================

B: 2951.61  {+/- 13.09}  sigmaB: 448.02

A: 189.93  {+/- 38.07}  sigmaA: 197.17

magDrop report: percentDrop: 93.6  magDrop: 2.979  +/- 0.218  (0.68 ci)

DNR: 6.16

D: 599.17 {+0.12,-0.11} (frame number)
D: [17:12:45.2556]  {+0.0062,-0.0057} seconds

R: 627.00 {+0.11,-0.12} (frame number)
R: [17:12:46.6470]  {+0.0057,-0.0062} seconds

Duration (R - D): 27.8273 {+0.1787,-0.1787} readings
Duration (R - D): 1.3914 {+0.0089,-0.0089} seconds

=============== end 0.68 containment interval report ===============

================= 0.95 containment interval report =================

B: 2951.61  {+/- 26.18}  sigmaB: 448.02

A: 189.93  {+/- 76.14}  sigmaA: 197.17

magDrop report: percentDrop: 93.6  magDrop: 2.979  +/- 0.435  (0.95 ci)

DNR: 6.16

D: 599.17 {+0.27,-0.29} (frame number)
D: [17:12:45.2556]  {+0.0133,-0.0143} seconds

R: 627.00 {+0.29,-0.27} (frame number)
R: [17:12:46.6470]  {+0.0143,-0.0133} seconds

Duration (R - D): 27.8273 {+0.3903,-0.3903} readings
Duration (R - D): 1.3914 {+0.0195,-0.0195} seconds

=============== end 0.95 containment interval report ===============

================= 0.9973 containment interval report ===============

B: 2951.61  {+/- 39.27}  sigmaB: 448.02

A: 189.93  {+/- 114.20}  sigmaA: 197.17

magDrop report: percentDrop: 93.6  magDrop: 2.979  +/- 0.653  (0.9973 ci)

DNR: 6.16

D: 599.17 {+0.55,-0.53} (frame number)
D: [17:12:45.2556]  {+0.0275,-0.0266} seconds

R: 627.00 {+0.53,-0.55} (frame number)
R: [17:12:46.6470]  {+0.0266,-0.0275} seconds

Duration (R - D): 27.8273 {+0.6956,-0.6956} readings
Duration (R - D): 1.3914 {+0.0348,-0.0348} seconds

=============== end 0.9973 containment interval report =============

D frame number: 599.17
D: 0.6800 containment intervals:  {+/- 0.12} (readings)
D: 0.9500 containment intervals:  {+/- 0.29} (readings)
D: 0.9973 containment intervals:  {+/- 0.55} (readings)

R frame number: 627.00
R: 0.6800 containment intervals:  {+/- 0.12} (readings)
R: 0.9500 containment intervals:  {+/- 0.29} (readings)
R: 0.9973 containment intervals:  {+/- 0.55} (readings)

Duration (R - D): 27.8273 readings
Duration: 0.6800 containment intervals:  {+/- 0.1787} (readings)
Duration: 0.9500 containment intervals:  {+/- 0.3903} (readings)
Duration: 0.9973 containment intervals:  {+/- 0.6956} (readings)

=============== Summary report for Excel file =====================

This light curve has not been block integrated.

This light curve has been normalized against a reference star.
... signal-track was used for normalization with X offset: 0
... 310 readings were used for smoothing



The observed drop has an estimated 40.9 sigma level of being a noise-induced-event

All times are calculated/reported based on the assumption that timestamps are start-of-exposure times.

It is critical that you make appropriate time adjustments when timestamps are NOT start-of-exposure times.
If you use the North American Excel Spreadsheet report, all times will be properly corrected
for camera delay and reported start-of-exposure times.
For other users worldwide, use the appropriate corrections documented in the North American Spreadsheet report form - use
the documentation shown on the Corrections Tables tab.

magDrop report: percentDrop: 93.6  magDrop: 2.979  +/- 0.435  (0.95 ci)

DNR: 6.16

D time: [17:12:45.2556]
D: 0.6800 containment intervals:  {+/- 0.0062} seconds
D: 0.9500 containment intervals:  {+/- 0.0143} seconds
D: 0.9973 containment intervals:  {+/- 0.0275} seconds

R time: [17:12:46.6470]
R: 0.6800 containment intervals:  {+/- 0.0062} seconds
R: 0.9500 containment intervals:  {+/- 0.0143} seconds
R: 0.9973 containment intervals:  {+/- 0.0275} seconds

Duration (R - D): 1.3914 seconds
Duration: 0.6800 containment intervals:  {+/- 0.0089} seconds
Duration: 0.9500 containment intervals:  {+/- 0.0195} seconds
Duration: 0.9973 containment intervals:  {+/- 0.0348} seconds

Enter D and R error bars for each containment interval in Excel spreadsheet without + or - sign (assumed to be +/-)

=========== end Summary report for Excel file =====================

Solution 'envelope' in the main plot drawn using 0.95 containment interval error bars

fit metrics for signal-Target

fit metrics === noiseSigmaDistance: 63.6

fit metrics === time error bar: +/- 0.0143 seconds

fit metrics === DNR: 6.16  
fit metrics === B: 2951.61  A: 189.93 sigmaB: 448.02  sigmaA: 197.17
fit metrics === magDrop report: percentDrop: 93.6  magDrop: 2.979  +/- 0.435  (0.95 ci)

fit metrics === D frame number: 599.1727

fit metrics === R frame number: 627.0000

fit metrics === duration: 1.3914 seconds

fit metrics === D time: [17:12:45.2556]

fit metrics === R time: [17:12:46.6470]




signal-Target is the target curve.

Data trimmed/selected using points: [392, 858]

signal-Target is the target curve.



#################### Session ended: Mon Dec  1 21:08:00 2025  ####################

